|  |
| --- |
| **Amerequip** **EU RoHS Compliance Declaration** |
| Part Number:       | Revision Level:       | Part Description:       |
| Supplier:       | Supplier Number:       |
| Supplier Contact:       | Phone:       | Email:       |
| **Reason For Submission:** \*Attach documentation as needed |
| [ ]  Initial Submission | [ ] \*Other – Please Specify:       |
| [ ]  Correction of Discrepancy (Resubmission) |
| **Submission Information:**  |
| Are all **Raw Materials** used in compliance with SPEC-C-Q005 Table 1?*\*Raw Material = bar stocks, sheet or plate, castings, molded components, etc.*[ ]  Yes [ ]  No (If No, explanation required)       |
| Are all **Ancillary Materials** used in compliance with SPEC-C-Q005 Table 1? *\*Ancillary = wires, hardware, clips, grommets, ties, hoses, fittings, etc.* [ ]  Yes [ ]  No (If No, explanation required)       |
| Are all **Indirect Materials** used in compliance with SPEC-C-Q005 Table 1? *\*Indirect = paints, thread locking compounds, weld wire, lubricants etc.* [ ]  Yes [ ]  No (If No, explanation required)       |
| **Chemical Substance Limits:** This table is for reference only. See SPEC-C-Q005 Table 1. |
| **Substance** | **Concentration Limit by Mass in Any Homogeneous Material** |
| Cadmium | 0.01% (100 ppm) |
| Lead | 0.1% (1000 ppm) |
| Mercury | 0.1% (1000 ppm) |
| Hexavalent Chromium | 0.1% (1000 ppm) |
| Polybrominated biphenyls (PBB) | 0.1% (1000 ppm) |
| Polybrominated diphenyl ethers (PBDE) | 0.1% (1000 ppm) |
| Bis (2-ethylhexyl) phthalate (DEHP) | 0.1% (1000 ppm) |
| Bis (2-ethylhexyl) phthalate (DEHP) | 0.1% (1000 ppm) |
| Butyl benzyl phthalate (BBP) | 0.1% (1000 ppm) |
| Dibutyl phthalate (DBP) | 0.1% (1000 ppm) |
| Disobutyl phthalate (DIBP) | 0.1% (1000 ppm) |
| **Amerequip EU RoHS Compliance Declaration Agreement:** |
| Name (printed):       | Title:       | Phone:       |
| Supplier Authorized Signature:       | Date:       |